"A)scii",1,IA,,,,,,0.92,,,,
"B)atch Ymodem (DSZ)",1,S,8,,B,1024,,0.90,,1=E,"C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] handshake slow estimate 0 [CBAUD] sb -k [FILE]","C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] handshake slow estimate 0 [CBAUD] rb [FILE] -p"
"C)rc Xmodem",1,IC,8,,,128,,0.78,,,,
"G) YmodemG (DSZ)",1,S,8,R,B,1024,,0.97,,1=E,"C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] handshake slow estimate 0 [CBAUD] sb -g [FILE]","C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] handshake slow estimate 0 [CBAUD] rb -g [FILE] -p"
"K)ermit",1,S,,,,128,F,0.78,,,"C:\RBBS\XFER\PCKERMIT.EXE -s [FILE] -l [PORT] -c -b [BAUD] -p [PARITY] -m 31","C:\RBBS\XFER\PCKERMIT.EXE -r -a [FILE] -l [PORT] -c -b [BAUD] -p [PARITY] -m 31"
"M)pt (formerly, PUMA)",1,S,8,,B,1024,,0.95,,1=E,"C:\RBBS\XFER\MPT.EXE S[BAUD] P[PORT#] HS LXFER-[NODE].DEF N+ A+ O- B- X+ S [FILE]","C:\RBBS\XFER\MPT.EXE S[BAUD] P[PORT#] HS LXFER-[NODE].DEF N+ A+ O- B- X+ R [FILE]"
"W)indowed Xmodem",1,S,,,,128,,0.78,,,"C:\RBBS\XFER\WXMODEM.COM -s -f [FILE] -l [PORT] -c -b [BAUD] -p W -n [NODE]","C:\RBBS\XFER\WXMODEM.COM -r -f [FILE] -l [PORT] -c -b [BAUD] -p W -n [NODE]"
"X)modem",1,IX,8,,,128,,0.78,,,,
"Y)modem (1K Xmodem)",1,IY,8,,,1024,,0.87,,,,
"Z)modem (Batch)",1,S,8,,B,1024,,0.95,,1=E,"C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] handshake slow estimate 0 [CBAUD] sz [FILE]","C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] handshake slow estimate 0 [CBAUD] rz [FILE] -p"
"N)one - Cancel

Select Protocol",1,IN,,,,,,,,,,
