"{C4{CS
",10,IN,,,,,,0.92,,,,
"A{C1) {C2- {C3ASCII Z-Modem Compression  (text only){C4
",10,S,8,,,1024,,0.95,,1=E,"C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] sz -Z -m [FILE]","C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] rz -Z -m -p [FILE]"
"K{C1) {C2- {C3Kermit{C4
",10,S,,,,128,F,0.78,,,"C:\RBBS\XFER\PCKERMIT.EXE -s [FILE] -l [PORT] -c -b [BAUD] -p [PARITY] -m 31","C:\RBBS\XFER\PCKERMIT.EXE -r -a [FILE] -l [PORT] -c -b [BAUD] -p [PARITY] -m 31"
"M{C1) {C2- {C3MPT/Puma{C4
",10,S,8,,B,1024,,0.95,,1=E,"C:\RBBS\XFER\MPT.EXE S[BAUD] P[PORT#] HS LXFER-[NODE].DEF N+ A+ O- B- X+ S [FILE]","C:\RBBS\XFER\MPT.EXE S[BAUD] P[PORT#] HS LXFER-[NODE].DEF N+ A+ O- B- X+ R [FILE]"
"X{C1) {C2- {C3X-Modem{C4
",10,S,8,,,512,,0.78,,1=E,"C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] sx [FILE]","C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] rx -p [FILE]"
"C{C1) {C2- {C3CRC X-Modem{C4
",10,S,8,,,512,,0.78,,1=E,"C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] sx [FILE]","C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] rx -p [FILE]"
"W{C1) {C2- {C3Windowed X-Modem{C4
",10,S,,,,128,,0.78,,,"C:\RBBS\XFER\WXMODEM.COM -s -f [FILE] -l [PORT] -c -b [BAUD] -p W -n [NODE]","C:\RBBS\XFER\WXMODEM.COM -r -f [FILE] -l [PORT] -c -b [BAUD] -p W -n [NODE]"
"Y{C1) {C2- {C3Y-Modem/1k  (1k X-Modem){C4
",10,S,8,,,1024,,0.82,,1=E,"C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] sx -k [FILE]","C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] rx -k -p [FILE]"
"B{C1) {C2- {C3Y-Modem  (True Y-Modem){C4
",10,S,8,,B,1024,,0.90,,1=E,"C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] sb -k [FILE]","C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] rb -p [FILE]"
"G{C1) {C2- {C3Y-Modem/G  (Reliable){C4
",10,S,8,R,B,1024,,0.95,,1=E,"C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] sb -g -k [FILE]","C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] rb -g -p [FILE]"
"H{C1) {C2- {C3HS-Link (not Bi-Directional){C4
",10,S,8,,B,4096,,0.93,,4=E=A,"C:\RBBS\XFER\HSLINK.EXE -@ -NF -NU -P[PORT#] -b[BAUD] -S4096 [FILE]","C:\RBBS\XFER\HSLINK.EXE -@ -NF -HX -UC:\RBBS\UPLOAD -P[PORT#] -b[BAUD] -s4096"
"Z{C1) {C2- {C3Z-Modem (CRC-16/24/32/MobyTurbo){C4
",10,S,8,,B,1024,,0.95,,1=E,"C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] sz -m [FILE]","C:\RBBS\XFER\DSZ.COM port [PORT#] speed [BAUD] estimate 0 [CBAUD] rz -m -p [FILE]"
"N{C1) {C2- {C4NONE {C3(cancel){C0

Select Protocol",10,IN,,,,,,,,,,

