InS_StArT
3C505.COM
1.0
^3Com 3C505 EtherLink+,3C505.COM,IE0
?The 3C505 EtherLink+ driver only supports operation in a 16-bit slot.
!RIE0(INT)Hardware Interrupt
@3
4
5
6
7
9
10
11
12
14
15
!RIE0(PORT)Base I/O Port
@300
310
320
330
340
350
360
370
380
390
3A0
!OIE0(DMA ) Optional DMA Channel
?DMA is optional for 3C505. If none is specified 3C505 will use PIO. If a DMA value is selected, the value must match the jumper setting on the board, and must be unique (not used by another device).   Recommended: No DMA for Windows.
5
6
7
$OIE0(NODE ADDRESS)Optional Node Address
0
7FFFFFFFFFFF
*RIE0(FRAME)Media Frame Type(s)
?Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
