InS_StArT
ILANAT.COM
1.0
^Racal-Datacom InterLan AT/XT ODI MLID,ILANAT.COM,IE0
!OIE0(PORT)
?The driver is self-configuring. If multiple ILanAT cards are in the system, specify an I/O base address.
300
320
340
360
380
3A0
3C0
3E0
$OIE0(NODE ADDRESS)
0
7FFFFFFFFFFF
*OIE0(FRAME)
?Note: Ethernet_802.2 is the default frame type for ODI drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_SNAP
Ethernet_II
InS_EnD
