InS_StArT
INTEL593.COM
1.0
^Intel593,INTEL593.COM,IE0
?This driver is used for systems compatible with the Intel LAN593 specification.  The LAN circuits can be either built directly into the system or onto an adapter board.
!OIE0(PORT)Base I/O Port
?This is optional. See your hardware documentation for the correct value.
@300 
310
320
330
340
350
360
370
!RIE0(INT)Interrupt Number
?This is optional.  See your hardware documentation for the correct value.
3
4
5
7
9
@10
11
12
15
!RIE0(DMA)DMA Channel 1
?This indicates the first DMA channel.
5
@6
7
!RIE0(DMA #2)DMA Channel 2
?This indicates the second DMA channel.
5
6
@7
*RIE0(FRAME)
?Note: Ethernet_802.2 is now the default frame type for ODI drivers.  Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
