InS_StArT
INTEL595.COM
1.0 
^Intel 82595 based Adapter,INTEL595.COM,IE0
?This is the DOS ODI driver of the Intel 82595 based adapter. It may be used in ISA or PCMCIA systems.
!OIE0(PORT)I/O Address
?Intel 82595 based adapters support the following I/O addresses: 200, 210, 220, 230, 240, 250, 260, 270, 300, 310, 320, 330, 340, 350, 360, 370. Run SOFTSET to change the I/O address setting.
200
210
220
230
240
250
260
270
@300
310
320
330
340
350
360
370
*RIE0(FRAME)Media Frame Type(s)
?Note: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
$OIE0(NODE ADDRESS)
?WARNING: Entering an incorrect value for NODE ADDRESS can cause serious network problems. If uncertain, LEAVE NODE ADDRESS BLANK.
0
FFFFFFFFFFFF
InS_EnD
