InS_StArT
LANSUP.COM
1.0
^ODI Module for the IBM LAN Support Program,LANSUP.COM,IEM
*OIEM()Primary or Alternate Adapter
?Set this parameter if the adapter is configured as an Alternate adapter.
ALTERNATE
$OIEM(SAPS)Number of SAPs
?The maximum number of SAPs that can be open at one time. The maximum number is 126 (125 for NETBIOS).
0
126
@1
!OIEM(LINK STATIONS)Number of Link Stations
?The maximum number of link stations that can be open at one time.
@1
*OIEM()RPL Reopen
?Set this parameter if are you using RPL to load LANSUP.COM
OPEN
$OIEM(MAX FRAME SIZE)Maximum Frame Size
?The maximum frame size must be a multiple of 8.
632
17960
@4208
InS_EnD
