c h a p t e r

Setting Up Additional Protocol Suppor t 31

Temp. Rev C - 1992

5 Setting Up Ad ditional Pr otocol

Suppor t

Chapter Ov erview

This chapter explains how to set up the workstation to use the Named Pipes protocol.

The following topics are in this chapter:

How to Use the Named Pipes Extender f or DOS

The Named Pipes extender for DOS is a terminate-and-stay-resident (TSR) program that extends the capability of DOS to include use of remote Named

Pipes. You must have an OS/2 Named Pipes server in order to use this extender.

This section explains how to install and con�gure the extender.

Topic Page

How to Use the Named Pipes Extender f or DOS 31

Loading the Extender into Memor y 32

Unloading the Extender from Memor y 32

Loading the Extender A utomatically 33

Con�gur ing the Named Pipes Extender 33

32 NetWare W orkstation f or DOS and Windo ws

Temp. Rev C - 1992

Prerequisite

The workstation on which you install the extender must be running DOS v3.3 or above.

Loading the Extender into Memor y

Your OS/2 workstation may require up to a minute after you run the extender for DOS before it is ready to run a Named Pipes application.

To load the extender, complete these steps:

1. Inser t the WSDOS_1 diskette into dr ive A:.

2. Change to dr ive A:.

3. Type the f ollowing:

DOSNP <Enter>

The extender is now loaded in memory.

4. Remo ve the disk ette .

5. If you want a repor t of the status of the Named Pipes e xtender , type the following at the DOS command line:

DOSNP /I <Enter>

Unloading the Extender from Memor y

To unload the extender, type the following at the DOS command line:

DOSNP /U <Enter>

Setting Up Additional Protocol Suppor t 33

Temp. Rev C - 1992

Loading the Extender A utomatically

To have the extender loaded into memory each time you boot your workstation, follow these steps:

1. Inser t the WSDOS_1 diskette into dr ive A:.

2. Copy the following �le to the boot dr ive (hard dr ive or �opp y diskette):

Copy A:\DOSNP.EXE

3. Add a line to y our AUTOEXEC.BAT �le that e xecutes the cop y of

DOSNP.EXE that y ou put on the boot dr ive.

This line should be placed after the line that loads IPX.COM and before the line that loads the DOS Requester (usually called VLM.EXE).

4. Remo ve the disk ette .

Each time you boot the workstation, the extender is loaded into memory.

Con�gur ing the Named Pipes Extender

You can use the NET.CFG �le to specify various options of the Named Pipes extender.

The following characteristics of the extender can be speci�ed in NET.CFG:

u Maximum machine names u Maximum open Named Pipes u Maximum communication buffers

Maximum Machine Names

Descr iption

Controls the number of Named Pipe servers with which the extender can communicate.

34 NetWare W orkstation f or DOS and Windo ws

Temp. Rev C - 1992

Syntax

NP MAX MACHINE NAMES = number

Replace number with how many named pipe servers you want cached on the

DOS machine.

Range: 4 to 50

Default: 10

Example

The following line in the NET.CFG �le changes the number of Named Pipes servers with which the workstation can communicate from 10 to 14:

NP MAX MACHINE NAMES= 14

Maximum Open Named Pipes

Descr iption

Speci�es the maximum number of Named Pipes the workstation can have open simultaneously.

Syntax

NP MAX OPEN NAMED PIPES = number

Replace number with the maximum number of Named Pipes that can be open simultaneously.

Range: 4 to 128

Default: 4

Example

The following line in NET.CFG changes the maximum number of pipes that the workstation can have open simultaneously from the default to 6:

NP MAX OPEN NAMED PIPES = 6

Setting Up Additional Protocol Suppor t 35

Temp. Rev C - 1992

Maximum Comm unication Buff ers

Descr iption

Speci�es the number of communication buffers that the extender can use to transmit data to and receive data from the Named Pipes server.

Syntax

NP MAX COMM BUFFERS = number

Replace number with the maximum number of communication buffers the extender can use to communicate with the Named Pipes server.

Range: 4 to 40

Default: 6

Example

The following line in the NET.CFG �le changes the number of communication buffers that the extender can use to communicate with the Named Pipes server from 6 to 10:

NP MAX COMM BUFFERS = 10

36 NetWare W orkstation f or DOS and Windo ws

Temp. Rev C - 1992