InS_StArT
E100ODI.COM
1.0
^Intel EtherExpress(tm) PRO/100 LAN Adapter,E100ODI.COM,IE0
?This is the DOS ODI driver for the Intel EtherExpress(tm) PRO/100 LAN adapter. It can be used with the Flash32 EISA / PCI or E100 EISA / PCI Adapters.
$OIE0(SLOT) Optional EISA - PCI Slot Num
?This DOSODI driver supports 15 EISA slots. For PCI, it signifies the Device ID shifted by 3 to mask off the function number. This parameter is optional.
1
15
$O000(FIFO) Optional FIFO Value
?Specify the FIFO threshold value to be used by the 82596 or 82556 LAN controller.
1
15
!O000(SCRAMBLE) Optional SCRAMBLE Enable
?Specify whether SCRAMBLING should be enabled or disabled in 100 Mbps operation.
0
1
$O000(THRESHOLD) Optional Tx Threshold
?Specify the Big-MAC transmit threshold.
0
200
!O000(PCIADAPTER) Optional PCI Adapter Type
?Specify which PCI adapter to install the driver on.
0
1
!O000(BUSARCH) Optional BUS Type
?Specify which BUS to select for the E100 adapter.
1
2
!O0E0(BURST) Optional PLX Burst Enable
?Specify whether the driver should enable BURST on the PLX EISA controller.
0
1
!O000(SPEED) Optional Line Speed
?Specify the data rate (line speed) of operation for the adapter. This is valid only for E100 adapters.
10
100
*O0E0(FRAME) Frame Type
?Note: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
$O0E0(NODE ADDRESS) Adapter Node Address
?Warning: Entering an incorrect value for the node address can cause serious network problems. If you are uncertain, leave the node address blank.
0
FFFFFFFFFFFF
InS_EnD
