BEGIN LeftB, MidB, RightB, LeftM, RightM, UpM, DownM
CHORDS menu1, menu1, menu1, menu2

LeftB:	TYPE ENTER
MidB:	TYPE 0, 46
RightB:	TYPE ESC

LeftM:	TYPE 0, 75
RightM:	TYPE 0, 77
UpM:	TYPE 0, 72
DownM:	TYPE 0, 80

	menu1:	MENU " TELIX COMMANDS ", 2, 25
		OPTION " DIALING DIRECTORY  ", dial
		OPTION "                    ",
		OPTION " Z-Modem DOWNload   ", zdown
 		OPTION " Z-Modem UPload     ", zup
		OPTION " Download Protocols ", down
		OPTION " Upload Protocols   ", up
		OPTION "                    ",
		OPTION " LOG Session        ", log
		OPTION " Jump to DOS        ", dos
		OPTION "                    ",
		OPTION " CHAT Mode          ", chat
		OPTION "                    ",
		OPTION " HANG UP MODEM      ", hang
		OPTION "                    ",
		OPTION " EXIT TELIX         ", exit
		MEND

	dial:	TYPE 0, 32
	zdown:	TYPE 0, 47, "rz", ENTER
	zup:	TYPE 0, 47, "sz ", 
	down:	TYPE 0, 81
	up:	TYPE 0, 73
	log:	TYPE 0, 38
	dos:	TYPE 0, 36
	chat:	TYPE 0, 21
	hang:	TYPE 0, 35
	exit:   TYPE 0, 45

	menu2:	MENU " PHONE DIRECTORY ", 5, 30, INVERSE
		OPTION " Number 1        ", d1
		OPTION " Number 2        ", d2
		OPTION " Number 3        ", d3
		OPTION " Number 4        ", d4
		OPTION " Number 5        ", d5
		OPTION " Number 6        ", d6
		OPTION " Number 7        ", d7
		OPTION " Number 8        ", d8
		OPTION " Number 9        ", d9
		OPTION " Number 10       ", d10
		MEND

	d1:	TYPE "1", ENTER
	d2:	TYPE "2", ENTER
	d3:	TYPE "3", ENTER
	d4:	TYPE "4", ENTER
	d5:	TYPE "5", ENTER
	d6:	TYPE "6", ENTER
	d7:	TYPE "7", ENTER
	d8:	TYPE "8", ENTER
	d9:	TYPE "9", ENTER
	d10:	TYPE "10, ENTER
