{ Epson MX-80 Printer Control and Print Modes}
{ D. Donohoe  6-22-85}

Const
{ These codes are for printer control. }
   Reset     =  #27#64;  { Resets all print modes, incl. TOP OF FORM.}
   Bell      =  #7;
   FF        =  #12;
   LF        =  #10;
   CR        =  #13;

{ These codes are the different print modes. }
{1} CompressOn = #15;       CompressOf = #15;      {Not with 5.           }
{2} DblWdthOn  = #14;       DblWdthOf  = #20;      {To end of line only.  }
{3} DblStrikOn = #27#71;    DblStrikOf = #27#72;   {                      }
{4} DblOn      = #27#87#1;  DblOf      = #27#87#0; {Stays on 'til cancelled}
{5} EmphOn     = #27#69;    EmphOf     = #27#70;   {Not with 1,7,8.       }
{6} ItalicsOn  = #27#52;    ItalicsOf  = #27#53;   {                      }
{7} SubOn      = #27#83#1;  SubOf      = #27#84;   {Not with 5.           }
{8} SuperOn    = #27#83#0;  SuperOf    = #27#84;   {Not with 5.           }
{9} UnderlinOn = #27#45#1;  UnderlinOf = #27#45#0; {                      }


