"B) Ymodem (ZSX - Batch - Both Directions)
9",5,D,8,,B,1024,,0.83,,4=E=A,"D:\RUTIL\ZSX.EXE port [PORT#] line [BAUD] log XFER-[NODE].DEF sb [FILE]","C:\RBBS\XFER\ZRB.BAT [PORT#] [BAUD] [NODE] [PROTO]"
"H) HS/Link -------- (One way or Bi-directional)
",4,D,8,,B,2048,,0.96,,4=E=A,"c:\rbbs\xfer\HS1DN.BAT [PORT#] [BAUD] [NODE] [PROTO] [FILE]","c:\rbbs\xfer\HS1UP.BAT [PORT#] [BAUD] [NODE] [PROTO] [FILE]"
"X) Xmodem (ZSX - Single File Uploading/Downloading)
9",5,D,8,,B,1024,,0.78,,4=E=A,"D:\RUTIL\ZSX.EXE port [PORT#] line [BAUD] log XFER-[NODE].DEF sx [FILE]","C:\RBBS\XFER\ZRX.BAT [PORT#] [BAUD] [NODE] [PROTO] [FILE]"
"Y) Ymodem  1K-Xmodem (ZSX)
9",5,D,8,,B,1024,,0.80,,4=E=A,"D:\RUTIL\ZSX.EXE port [PORT#] line [BAUD] log XFER-[NODE].DEF sy [FILE]","C:\RBBS\XFER\ZRY.BAT [PORT#] [BAUD] [NODE] [PROTO] [FILE]"
"Z) Zmodem (ZSX)
9",5,D,8,,B,1024,,0.94,,4=E=A,"D:\RUTIL\ZSX.EXE port [PORT#] line [BAUD] log XFER-[NODE].DEF sz [FILE]","C:\RBBS\XFER\ZRZ.BAT [PORT#] [BAUD] [NODE] [PROTO]"
"N)one - Cancel

Select Protocol",1,IN,,,,,,,,,,
