
  OS/2 2.x .ADD driver for Creative Labs CD.

  This driver is the official driver for the older Panasonic 521
  and ALSO for the new Panasonic 562/563 drive

  under 2.1 you need the DEVICE=OS2CDROM.DMD and IFS=CDFS.IFS
  installed, then add BASEDEV=SBCD2.ADD, /P:xxx where .ADD file
  MUST be in the ROOT of the boot drive OR the OS2 subdirectory
  and xxx is the address of your SBPro or SB16.

  If you are installing OS/2 2.1 from CD, then

  copy the SBCD2.ADD to DISKETTE 1
  edit the CONFIG.SYS on diskette 1 and add the following line
  BASEDEV=SBCD2.ADD /P:xxx

  insert the CD in the CD drive
  and boot the two diskettes.

  IMPORTANT UPDATE
  IMPORTANT UPDATE
  IMPORTANT UPDATE
  IMPORTANT UPDATE

  There is a bug in OS/2 2.1 install from CD.
  The CD support files are NOT installed on the
  hardfile. SO, after boot for the final time,
  at the workpace shell, copy OS2CDROM.DMD and
  CDFS.IFS from DISKETTE 1 to your OS2 subdirectory
  and add the following two lines to your config.sys

  DEVICE=x:\OS2\OS2CDROM.DMD /Q
  IFS=x:\OS2\CDFS.IFS /Q

  where x: = your boot drive (D: for example)


