
========================================================================
         SETUP FOR SUPRAFAX V32BIS EXTERNAL MODEM AT 1:352/111
                       USING BGFAX140B AND FD212
========================================================================

[FDSETUP] Modem -> Default Settings -> Command Strings
  Init-1 ... atz|
  Init-2 ... at+fcr=1;+fdcc=1,5,0,2,0,0,0,0|
  Init-3 ... at+flid="360 427 1123"|
  Delay  ... 2

[FDSETUP] Modem -> Default Settings -> Answer control
  Manual answer ... Yes
  Force answer  ... at+faa=1;a|
  Answer delay  ... 40

[FDSETUP] Modem -> Default Settings -> Connect messages
  Fax ... FAX


[BBS.BAT] NOTE: set errorlevel at 255 for maximum speed!
...
IF ERRORLEVEL 255 GOTO FAX
...
:FAX
C:
CD \BBS\FAX
BGFAX.EXE /FAX C:\BBS\FAX\FAX-IN 1 Q /NF
ECHO. >> C:\BBS\FAX\FAX.LOG
LOGECHO ----------  $W $D $N $Y, BGFax >> C:\BBS\FAX\FAX.LOG
LOGECHO * $h:$m:$s  Incoming FAX Received >> C:\BBS\FAX\FAX.LOG
GOTO FDSTART

[AUTOEXEC.BAT]
C:\BBS\FAX\NFAX.COM

=============================================================================
                    SUPRAFAX V32BIS MODEM AT 1:352/111
=============================================================================

ACTIVE PROFILE:
B1 E1 L2 M1 N1 Q0 T V1 W2 X4 Y0 %C0 %E0 %G0 \N3 &C1 &D2 &K3 &Q5 &R0 &S0 &X0 &Y0
S00:000 S01:000 S02:043 S03:013 S04:010 S05:008 S06:002 S07:090 S08:002 S09:020
S10:060 S11:050 S12:050 S18:000 S23:063 S25:005 S26:001 S36:007 S37:011 S38:020
S40:119 S46:138 S48:007 S91:009 S95:003 S109:062 S110:001 

STORED PROFILE 0:
B1 E1 L2 M1 N1 Q0 T V1 W2 X4 Y0 %C0 %E0 %G0 \N3 &C1 &D2 &K3 &Q5 &R0 &S0 &X0 
S00:000 S02:043 S06:002 S07:090 S08:002 S09:020 S10:060 S11:050 S12:050 S18:000
S23:063 S25:005 S26:001 S36:007 S37:011 S38:020 S40:119 S46:138 S48:007 S95:003

STORED PROFILE 1:
B1 E1 L2 M0 N1 Q0 T V1 W1 X4 Y0 %C1 %E0 %G1 \N3 &C1 &D2 &K3 &Q5 &R0 &S0 &X0 
S00:000 S02:043 S06:002 S07:050 S08:002 S09:006 S10:014 S11:095 S12:050 S18:000
S23:061 S25:005 S26:001 S36:007 S37:000 S38:020 S40:087 S46:138 S48:007 S95:000

TELEPHONE NUMBERS:
0=                                      1=
2=                                      3=
