e:                      ; drive letter of cdrom player
c:\pcsig\tempdir        ; temp drive for compressed or xfer files
c:\pcsig                ; where cdcom will be located
on                      ; bell on/off when paged
1000                    ; lowest security allowed to drop into dos
gate1                   ; Redirected output when compressing (not used)
1_2804.upp              ; path\filename to descriptions
c:\pcsig                ; path for log file
50                      ; minumum security allowed to download
n                       ; send files from cdrom (y), copy to tempdir (n)
n                       ; reboot system if cdrom timeout
N                       ; allow auto-logoff
c:\pcsig                ; path to missing disks
Y                       ; add ----- to log file
1,36,40                 ; normal text
1,37,40                 ; high lighted text
n                       ; 10th edition Y, all others N
2804                    ; # of disk numbers on disk
