





                              BYTE/WIDE Software, Inc. 

                                        ZMENU

                         "QUICK START" Instruction procedure


              *** Follow these simple instructions for installing ZMENU ***


               First change your "logged" disk drive to the "A" drive. 
          This is the drive you will use to install ZMENU from.

               The screen should look like this:  A>


               To change drives, (log to a drive) if necessary, simply type
          in the drive letter you want (which is "A") followed by a colon
          at the system prompt and press the 'RETURN' key.

               C>A: <CR>      <CR> - means press the 'RETURN' key
                    gives you
               A> 


               Next insert the ZMENU system diskette into the floppy disk
          drive ("A") and, at the system prompt type in "INSTALL" then
          press the 'RETURN' key.  NOTE: the floppy disk must be drive "A".

               A>INSTALL <CR>


               At this point, the Install program will guild you throw the
          User agreement and Loading of ZMENU menu system.  NOTE: ZMENU
          will not run if the User agreement is not met properly.


               ZMENU is not copy protected, so it will not conflict with
          the Backup programs.


               When installation is complete ZMENU will load and startup 
          automatically to the MAIN MENU.




          MORE NOTES:
               The ZMENU manual and registration card are on disk, to print
          your copy just enter the submenu of 'DOS' and select the option
          for 'PRINT ZMENU MANUAL'.



