                  Printer definition file for WSSINDEX

All lines of this file are comments until a line beginning ----.  After that,
alternate lines are comments and parameters.  See the WSSINDEX documentation
for a description of the format allowed here.  Commands in this file are for an
HP Laser Jet II.  Contributed by Dorothy Hair, typed in and commented by RWB.

Commands used in this file:

  27 69           = \e E             = reset
  27 38 108 49 69 = \e & l \1 E      = 1 line top margin
      (contributed file had 1 rather than 49 or \1, but I think that's wrong)
  27 38 108 56 52 70 = \e & l \8\4 F = 84 lines per page
  27 38 107 50 83 = \e & k \2 S      = 16.66 pitch
  27 38 108 56 68 = \e & l \8 D      = 8 lines per inch
  12              = \f               = form feed

These command strings have been tested using DUMPPCL by Brian K. Uechi.
------------------------------------------------------------
Printer name
HP Laser Jet II
Optional string printed on all labels
Property of <your name here>
Printer initialization command for 1,2,... column printing, 50 max
\e E, \e & l \1 E, \e & l \8\4 F
Printer initialization command for labels, 50 max (pitch, line spacing, etc.)
\e & k \2 S, \e & l \8 D
Printer initialization command for disk covers, 50 max
\e & k \2 S, \e & l \8 D
Printer deinitialization command, 10 max (form feed for laser printer, etc.)
\f
Number of spaces in left margin for labels
5
Number of columns for labels
2
Width of labels (characters)
50
Number of characters between labels (if multiple columns)
3
Length of label in lines (including unusable lines)
12
Number of usable lines for label
9
Number of spaces in left margin for disk covers
9
Width of paper for disk covers (characters)
90
Length of page in lines for disk covers
40
Printer command to position for the next disk cover

Character to use for sides of disk cover box (32 = blank prints faster)
186
Character to use for top and bottom lines
205
Character to use for top left corner
201
Character to use for top right corner
187
Character to use for bottom left corner
200
Character to use for bottom right corner
188
End of printer configuration file
