                  Printer definition file for WSSINDEX

All lines of this file are comments until a line beginning ----.  After that,
alternate lines are comments and parameters.  Printer control sequences and
other items (except for the printer name and label id string) are ascii
characters, decimal numbers, octal numbers, hexadecimal number or special
sequences preceded by a \, separated by commas or spaces.  The codes in this
file are for screen display, not for a printer.
------------------------------------------------------------
Printer name
IBM screen characters
Optional string printed on all labels
Property of <your name here>
Printer initialization command for 1,2,... column printing, 50 max

Printer initialization command for labels, 50 max (pitch, line spacing, etc.)

Printer initialization command for disk covers, 50 max

Printer deinitialization command, 10 max (form feed for laser printer, etc.)

Number of spaces in left margin for labels
5
Number of columns for labels
1
Width of labels (characters)
50
Number of characters between labels (if multiple columns)
5
Length of label in lines (including unusable lines)
12
Number of usable lines for label
9
Number of spaces in left margin for disk covers
0
Width of paper for disk covers (characters)
79
Length of page in lines for disk covers
40
Printer command to position for the next disk cover

Character to use for sides of disk cover box (32 = blank prints faster)
0xba
Character to use for top and bottom lines
0xcd
Character to use for top left corner
0xc9
Character to use for top right corner
0xbb
Character to use for bottom left corner
0xc8
Character to use for bottom right corner
0xbc
End of printer configuration file
