                  Printer definition file for WSSINDEX

All lines of this file are comments until a line beginning ----.  After that,
alternate lines are comments and parameters.  See the WSSINDEX documentation
for a description of the format allowed here.

Contributed by Ken Barney, typed in by RWB.

Commands used in this file:

  27 64    = \e @    = reset
  27 65 6  = \e A 6  = define 6/72 inch line feed (12 lines per inch)
  27 50    = \e \2   = use the 12 lpi defined by \e A above
  27 83 48 = \e S \0 = select superscript mode (0 instead of \0 also works)
------------------------------------------------------------
Printer name
Star LV-1210
Optional string printed on all labels
Property of <your name here>
Printer initialization command for 1,2,... column printing, 50 max

Printer initialization command for labels, 50 max (pitch, line spacing, etc.)
27 64 27 65 6 27 50 27 83 48
Printer initialization command for disk covers, 50 max
27 64 27 65 6 27 50 27 83 48
Printer deinitialization command, 10 max (form feed for laser printer, etc.)
27,64
Number of spaces in left margin for labels
5
Number of columns for labels
1
Width of labels (characters)
50
Number of characters between labels (if multiple columns)
5
Length of label in lines (including unusable lines)
12
Number of usable lines for label
9
Number of spaces in left margin for disk covers
0
Width of paper for disk covers (characters)
50
Length of page in lines for disk covers
30
Printer command to position for the next disk cover
10 10 10 10
Character to use for sides of disk cover box (32 = blank prints faster)
186
Character to use for top and bottom lines
205
Character to use for top left corner
201
Character to use for top right corner
187
Character to use for bottom left corner
200
Character to use for bottom right corner
188
End of printer configuration file
