                  Printer definition file for WSSINDEX

All lines of this file are comments until a line beginning ----.  After that,
alternate lines are comments and parameters.  See the WSSINDEX documentation
for a description of the format allowed here.

Commands used:
\e ~ E 0 1 1   select IBM Proprinter mode
\e I 3         select 10 cpi Courier letter quality (lq) font
15             turn on compressed print (can't get lq in compressed mode)
\e S 0         turn on superscripting (to get smaller characters)
\e T           turn off superscripting
\e \3 27       8 lines per inch (27/216=1/8)
\e \3 18       12 lines per inch (18/216=1/12)
18             select 10 cpi
\e P 0         proportional spacing off

For wider box forming characters, use
 ---  ---  ---                ---  ---  ---
| 201 205 187 |              | 218 196 191 |
| 186     186 |  instead of  | 179     179 |
| 200 205 188 |              | 192 196 217 |
 ---  ---  ---                ---  ---  ---

I don't know what selecting superscript mode does to the number of charcters
per inch, so the widths for labels and covers may need to be adjusted.

Entered 1/22/90 by RWB from a donated copy of a Toshiba manual.  Box forming
characters from Word Perfect printer driver.
------------------------------------------------------------
Printer name
Toshiba 321SL in IBM Proprinter mode (untested)
Optional string printed on all labels
Property of <your name here>
Printer initialization command for 1,2,... column printing, 50 max
\e ~ E 0 1 1, \e P 0, \e I 3
Printer initialization command for labels, 50 max (pitch, line spacing, etc.)
\e ~ E 0 1 1, 15, \e P 0, \e S 0, \e \3 18
Printer initialization command for disk covers, 50 max
\e ~ E 0 1 1, 15, \e P 0, \e S 0, \e \3 27
Printer deinitialization command, 10 max (form feed for laser printer, etc.)
\e T, 18
Number of spaces in left margin for labels
5
Number of columns for labels
1
Width of labels (characters)
50
Number of characters between labels (if multiple columns)
5
Length of label in lines (including unusable lines)
12
Number of usable lines for label
9
Number of spaces in left margin for disk covers
0
Width of paper for disk covers (characters)
82
Length of page in lines for disk covers
40
Printer command to position for the next disk cover
10 10 10 10
Character to use for sides of disk cover box (32 = blank prints faster)
179
Character to use for top and bottom lines
196
Character to use for top left corner
218
Character to use for top right corner
191
Character to use for bottom left corner
192
Character to use for bottom right corner
217
End of printer configuration file
