                  Printer definition file for WSSINDEX

All lines of this file are comments until a line beginning ----.  After that,
alternate lines are comments and parameters.  See the WSSINDEX documentation
for a description of the format allowed here.  The codes in this file are for
a Citoh Tri Printer model 20 dot matrix printer.  To make it easier for
people to read the printer sequences, I have used blanks to separate
characters, and commas to separate multi-character printer commands.  Most of
these delimiters are not required by the routine which reads this file.

Commands (not all used in this file):

  \e a \2   = 6 lines per inch
  \e a \3   = 8 lines per inch
  \e a \5   = 12 lines per inch
  \e S 0    = superscript mode
  \e P      = 10 cpi
  \e M      = 12 cpi
  \e c      = compressed print (16.5 or 17.1 cpi, apparently only selectable
              from the printer control panel)
  \e + \1   = letter quality mode
  \e @      = reset
Created using manual pages donated by J. Fabrizio.
Untested.  In particular, I don't know whether the box-forming characters
will work.
------------------------------------------------------------
Printer name
Citoh Tri Printer Model 20
Optional string printed on all labels
Property of <your name here>
Printer initialization command for 1,2,... column printing, 50 max
\e + \1
Printer initialization command for labels, 50 max (pitch, line spacing, etc.)
\e + \1,\e M,\e S 0,\e c
Printer initialization command for disk covers, 50 max
\e + \1,\e a 3,\e c
Printer deinitialization command, 10 max (form feed for laser printer, etc.)
\e @
Number of spaces in left margin for labels
5
Number of columns for labels
1
Width of labels (characters)
50
Number of characters between labels (if multiple columns)
5
Length of label in lines (including unusable lines)
12
Number of usable lines for label
9
Number of spaces in left margin for disk covers
0
Width of paper for disk covers (characters)
90
Length of page in lines for disk covers
40
Printer command to position for the next disk cover
10 10 10 10
Character to use for sides of disk cover box (32 = blank prints faster)
245
Character to use for top and bottom lines
241
Character to use for top left corner
240
Character to use for top right corner
242
Character to use for bottom left corner
246
Character to use for bottom right corner
247
End of printer configuration file
