; ---------
; Epson.def
; ---------
; These definitions should work at least for the following printers:
;     Epson FX-80/100           -- **untested**
;     Epson LX-80               -- **untested**
;     IBM Graphics Printer      -- **untested**
;     Panasonic KX-P1081        -- tested
;
Init            "\e@"
Pitch(10)       "\eP"
Pitch(12)       "\eM"
Pitch(17)       "\eP\x0F"
;
; Quality changing--these commands are for the Panasonic KX-P1081,
; and I don't know whether or not they work with the Epsons.
;
; Quality(0)      "\ex0"
; Quality(2)      "\ex1"
;
Spacing(2)      "\e3l"
Spacing(3)      "\e3H"
Spacing(4)      "\e36"
Spacing(6)      "\e3$"
Spacing(8)      "\e3\e"
Term            ""
